Commands:

* Pause clock
* Resume clock
* Step one instruction
* Read signal
* Write to memory
* Read register
* Read memory

Signals to be read: